Firmware version: 0013.0003

Firmware files:

JTH5500_UN108v01.bin
JTH5501_UN108v01.bin


-------------------------------------------------------------------------------------

What's new:

FW 0013.0003
1. Fixed fonts display leak issue when switching to DSLR HDMI display.

-------------------------------------------------------------------------------------

History updates:

FW 0011.0003
1. Signal format displays 59.94 instead of 60. 
2. Default color temperature changed to "Native"
3. Signal format display and battery info display can be individually turned on/off.
4. Support 17^3, 33^3, 65^3 User Lut cube upload
5. Add Ħ°SaturationĦħ adjustment in calibration menu.
6. Fixed audio meter bug
7. Add start-up background image instead of black screen
8. Compatible with Kinefinity camera 
9. Joystick down: quick adjust backlight
10. Joystick long down: delete current scene



-------------------------------------------------------------------------------------

Upgrade steps

Tool: SD card, FAT32
Step:
1. Unzip the firmware pack, copy JTH5500_UN108v01.bin and JTH5501_UN108v01.bin to SD card, root directory. (Do not rename any files)
2. Insert SD card to the monitor, and switch on the monitor.
3. Hold the joystick long Left, to enter Menu
4. Select: System ¨CFIRMWARE UPDATE, and follow the OSD instructions to update.
Caution: Please make sure the power is not cut off during update.



-------------------------------------------------------------------------------------


